2004/11/16 INPROCOMM release note
P.S H/W Sample's label will show T60N871.00 XXXXX-04

[Toshiba Home Model]
Release PCI for 2K/XP

Driver version:  3.3.11.2004 
1.Driver v3.3.11.2004  WHQL'd driver.
2.It won't Install UI in WinXP.By default,we use XP WZC.
3.Fix Rx sensitivity issue.
4.Running Slient Install. You need to open a dos mode window.
  type the following command:
  For example.   setup /s -f1"c:\temp\Slient_Install_20040924\setup.iss"
5.Change PCI_Vendor_Device_ID to 17FE222003101468 from 17FE2220222017FE.
  (Foxconn assigned an ID:[03101468] for Toshiba.)
6.Fix S1/S3 halt issue on Toshiba EW3 notebook PC.
7.Pass HCT.12 fully test.


Utility version: v1.17.11.2004.(Only installed UI in Windows 2000.
Don't need UI of Toshiba Home Model.

IEEE 802.1x Supplicant protocol driver version: 1.06.11.2004

IEEE 802.1x Supplicant protocol driver version: 1.05.11.2004
1.Add notification to UI if the opened adapter's power mode is changed from D3 to D0.

IEEE 802.1x Supplicant protocol driver version: 1.04.10.2004
1.Fix the bug that system will crash if user closes protocol service after close UI without
  close the opened adapter ahead.
2.Change indication if user disable/remove current opened adapter.

###########################################################################
2004/11/13 INPROCOMM release note
P.S H/W Sample's label will show T60N871.00 XXXXX-04

[Toshiba Home Model]
Release PCI for 2K/XP

Driver version:  3.3.11.2004 
1.Driver v3.3.11.2004  non-pass WHQL.
2.It won't Install UI in WinXP.By default,we use XP WZC.
3.Fix Rx sensitivity issue.
4.Running Slient Install. You need to open a dos mode window.
  type the following command:
  For example.   setup /s -f1"c:\temp\Slient_Install_20040924\setup.iss"
5.Change PCI_Vendor_Device_ID to 17FE222003101468 from 17FE2220222017FE.
  (Foxconn assigned an ID:[03101468] for Toshiba.)
6.Fix S1/S3 halt issue on Toshiba EW3 notebook PC.
7.Pass HCT.12 fully test.


Utility version: v1.17.11.2004.(Only installed UI in Windows 2000.
Don't need UI of Toshiba Home Model.

IEEE 802.1x Supplicant protocol driver version: 1.06.11.2004

IEEE 802.1x Supplicant protocol driver version: 1.05.11.2004
1.Add notification to UI if the opened adapter's power mode is changed from D3 to D0.

IEEE 802.1x Supplicant protocol driver version: 1.04.10.2004
1.Fix the bug that system will crash if user closes protocol service after close UI without
  close the opened adapter ahead.
2.Change indication if user disable/remove current opened adapter.

###########################################################################
2004/11/09 INPROCOMM release note
P.S H/W Sample's label will show T60N871.00 XXXXX-04

[Toshiba Home Model]
Release PCI for 2K/XP

Driver version:  3.3.11.2004 
1.Driver v3.3.11.2004  non-pass WHQL.
2.It won't Install UI in WinXP.By default,we use XP WZC.
3.Fix Rx sensitivity issue.
4.Running Slient Install. You need to open a dos mode window.
  type the following command:
  For example.   setup /s -f1"c:\temp\Slient_Install_20040924\setup.iss"
5.Change PCI_Vendor_Device_ID to 17FE222003101468 from 17FE2220222017FE.
  (Foxconn assigned an ID:[03101468] for Toshiba.)
6.Fix S1/S3 halt issue on Toshiba EW3 notebook PC.
7.Pass HCT.12 fully test.


Utility version: N/A.(Only installed UI in Windows 2000.
Don't need UI of Toshiba Home Model.

IEEE 802.1x Supplicant protocol driver version: 1.05.11.2004
1.Add notification to UI if the opened adapter's power mode is changed from D3 to D0.

IEEE 802.1x Supplicant protocol driver version: 1.04.10.2004
1.Fix the bug that system will crash if user closes protocol service after close UI without
  close the opened adapter ahead.
2.Change indication if user disable/remove current opened adapter.

###########################################################################
2004/10/27 INPROCOMM release note
P.S H/W Sample's label will show T60N871.00 XXXXX-04

[Toshiba Home Model]
Release PCI for 2K/XP

Driver version:  3.2.10.2004 
1.Driver v3.2.10.2004  non-pass WHQL.
2.It won't Install UI in WinXP.By default,we use XP WZC.
3.Fix Rx sensitivity issue.
4.Running Slient Install. You need to open a dos mode window.
  type the following command:
  For example.   setup /s -f1"c:\temp\Slient_Install_20040924\setup.iss"
5.Change PCI_Vendor_Device_ID to 17FE222003101468 from 17FE2220222017FE.
  (Foxconn assigned an ID:[03101468] for Toshiba.)
6.Pass HCT.12 test.
7.Fix S1/S3 halt issue on Toshiba EW3 notebook PC.


Utility version: N/A.
Don't need UI of Toshiba Home Model.